After discussions with the president of the Pilots’ Association and the chairman of the Mariners’ Advisory Committee, we have decided on the following temporary guidelines for outbound deep draft vessels (37’-40’). These windows are intended to maximize the use of the available water when transiting the New Castle and Deepwater ranges. Following the completion of maintenance dredging, these temporary guidelines will be re-evaluated and changes will be made as necessary.

**37’ - 40’ outbound from Packer Avenue including Beckett Street**

- Use reference station Philadelphia.

- Vessels may sail 3 hours before low water and up until 1.5 hours after low water at Philadelphia.

**37’ - 40’ outbound from Paulsboro**

- Please use reference station Marcus Hook.

- Vessels may sail from Paulsboro 1 hour before low water up until 3 hours after low water at Marcus Hook.

**37’ - 40’ outbound from Marcus Hook (anchorage or berth)**  
- Please use reference station Marcus Hook.

- Vessels may sail 1 hour after low water up until high water at Marcus Hook.

- **All inbound vessels over 37’6” will transit on flood tide only.**